<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="78.9" y2="0" width="0" layer="20"/>
<wire x1="78.9" y1="0" x2="78.9" y2="100" width="0" layer="20"/>
<wire x1="78.9" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<text>Pure MIDI v1.1</text>
<text>jhbruhn 2019</text>
<hole x="17.272" y="22.86" drill="3.2"/>
<hole x="17.272" y="3.048" drill="3.2"/>
<hole x="17.272" y="34.544" drill="3.2"/>
</plain>
<libraries>
<library name="thonkiconn">
<packages>
<package name="WQP-PJ301M-12_JACK">
</package>
</packages>
</library>
<library name="yarns_v03">
<description>Generated from &lt;b&gt;yarns_v03.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="OG-MIDI_SD-50BV">
</package>
</packages>
</library>
<library name="GMSN">
<packages>
<package name="2X5-SHROUDED">
</package>
</packages>
</library>
<library name="con-kycon">
<description>&lt;b&gt;Connector from KYCON, Inc&lt;/b&gt;&lt;p&gt;
1810 Little Orchard Street,&lt;br&gt;
San Jose,&lt;br&gt;
CA 95125 (408)494-0330&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/autor&gt;</description>
<packages>
<package name="KUSBVX-BS1N">
<description>&lt;b&gt;USB B-type Receptacle&lt;/b&gt; Vertical, 4 Position, Through Hole&lt;p&gt;
Source: Sibalco Kycon KUSBVX-BS1N-xxx.pdf</description>
</package>
</packages>
</library>
<library name="AD5676ARUZ">
<packages>
<package name="RU_20">
</package>
</packages>
</library>
<library name="switch-alps">
<description>ALPS Switch from Markus Faust &amp;lt;mfaust@htwm.de&amp;gt;&lt;p&gt;
Source: EC12E.scr from eagle.support.ger on news.cadsoft.de at 08.10.2007</description>
<packages>
<package name="ALPS_EC12E_SW">
<description>ALPS rotary encoder&lt;br&gt;
EC12E series with push-on switch</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="C1_ADAFRUIT_1.3_128X64_OLED">
<description>Package generated by &lt;b&gt;make-group2pac.ulp&lt;/b&gt;&lt;p&gt; from: /home/jhbruhn/Downloads/Adafruit_1.3_128x64_OLED.brd&lt;br&gt; at: 31.07.19 00:18</description>
</package>
</packages>
</library>
<library name="6n138">
<packages>
<package name="SO8-GW300">
<description>&lt;b&gt;HCPL-772X Package witch Gull Wing Surface Mount Option 300&lt;/b&gt;&lt;p&gt;
Source: HCPL7221.pdf</description>
</package>
</packages>
</library>
<library name="ad5754">
<packages>
<package name="RE_24">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-PTH-1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 2x5 ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://portal.fciconnect.com/Comergent//fci/drawing/20021111.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="og-stm32f2">
<packages>
<package name="LQFP48">
</package>
</packages>
</library>
<library name="analog-adr43x">
<packages>
<package name="MSOP8">
<description>&lt;b&gt;Micro Small Outline Package&lt;/b&gt; Grid .65mm&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="jhbruhn-opamp">
<packages>
<package name="SOIC8">
<description>&lt;b&gt;Small Outline IC&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jhbruhn-cdr">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="CASE-A_3216">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 reflow solder&lt;/b&gt;&lt;p&gt;KEMET S / EIA 3216-12</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
<package name="NX5032">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R7" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X4" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X5" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X6" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X11" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X12" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X13" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X14" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="C3" library="jhbruhn-cdr" package="C0603" value="22p">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="jhbruhn-cdr" package="C0603" value="22p">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="jhbruhn-cdr" package="R0603" value="220R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="jhbruhn-cdr" package="SOD123" value="1N4148W">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="jhbruhn-cdr" package="R0603" value="470R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="X21" library="yarns_v03" package="OG-MIDI_SD-50BV" value="OG-MIDI_MAB5SHCUI-SD-50BV">
<attribute name="NAME"/>
</element>
<element name="R19" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="PWR1" library="GMSN" package="2X5-SHROUDED" value="HEADER2X5SHD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="jhbruhn-cdr" package="SOD123" value="B5819W">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="jhbruhn-cdr" package="SOD123" value="B5819W">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="jhbruhn-cdr" package="CASE-A_3216" value="10uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C19" library="jhbruhn-cdr" package="CASE-A_3216" value="10uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C20" library="jhbruhn-cdr" package="CASE-A_3216" value="10uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C9" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="X22" library="yarns_v03" package="OG-MIDI_SD-50BV" value="OG-MIDI_MAB5SHCUI-SD-50BV">
<attribute name="NAME"/>
</element>
<element name="U2" library="AD5676ARUZ" package="RU_20" value="AD5676ARUZ">
<attribute name="NAME"/>
</element>
<element name="X2" library="con-kycon" package="KUSBVX-BS1N" value="KUSBVX-BS1N">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X8" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X9" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X10" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X17" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X18" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X19" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X20" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="R10" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="X15" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="X16" library="thonkiconn" package="WQP-PJ301M-12_JACK" value="WQP-PJ301M-12_JACK">
<attribute name="NAME"/>
</element>
<element name="R16" library="jhbruhn-cdr" package="R0603" value="51R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="jhbruhn-cdr" package="R0603" value="51R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="jhbruhn-cdr" package="R0603" value="22R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="jhbruhn-cdr" package="R0603" value="22R">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="switch-alps" package="ALPS_EC12E_SW" value="EC12E_SW">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EC12E2424407"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1520813"/>
<attribute name="OC_NEWARK" value="74M1068"/>
<attribute name="POPULARITY" value="3"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="microbuilder" package="C1_ADAFRUIT_1.3_128X64_OLED" value="OLED_1.3_128X64_SPI"/>
<element name="IC5" library="6n138" package="SO8-GW300" value="6N138SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="ad5754" package="RE_24" value="AD5754BREZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="AD5754BREZ"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Vendor"/>
</element>
<element name="C11" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X5-PTH-1.27MM" value="CORTEX_DEBUG_PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="jhbruhn-cdr" package="R0603" value="1k5">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="v-reg" package="SOT223" value="LD117AS33TR">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="9"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="IC1" library="og-stm32f2" package="LQFP48" value="STM32F373C">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="jhbruhn-cdr" package="CASE-A_3216" value="10uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="SPICEPREFIX" value="C"/>
</element>
<element name="C25" library="jhbruhn-cdr" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="jhbruhn-cdr" package="R0603" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="jhbruhn-cdr" package="R0603" value="39k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="jhbruhn-cdr" package="R0603" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="jhbruhn-cdr" package="R0603" value="39k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="jhbruhn-cdr" package="R0603" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="jhbruhn-cdr" package="R0603" value="39k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="jhbruhn-cdr" package="R0603" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="jhbruhn-cdr" package="R0603" value="39k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="jhbruhn-cdr" package="R0603" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="jhbruhn-cdr" package="R0603" value="39k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="jhbruhn-cdr" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="jhbruhn-cdr" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="jhbruhn-cdr" package="R0603" value="56k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="jhbruhn-cdr" package="R0603" value="39k">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="70"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="jhbruhn-opamp" package="SOIC8" value="TL072CD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="analog-adr43x" package="MSOP8" value="ADR435">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="analog-adr43x" package="MSOP8" value="ADR431">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="jhbruhn-opamp" package="SOIC8" value="TL072CD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="jhbruhn-opamp" package="SOIC8" value="TL072CD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="jhbruhn-cdr" package="C0603" value="100n">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="73"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="jhbruhn-cdr" package="NX5032" value="8MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R19" pad="1"/>
<contactref element="C20" pad="-"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="X6" pad="P$3"/>
<contactref element="X3" pad="P$3"/>
<contactref element="X4" pad="P$3"/>
<contactref element="X5" pad="P$3"/>
<contactref element="X11" pad="P$3"/>
<contactref element="X12" pad="P$3"/>
<contactref element="X13" pad="P$3"/>
<contactref element="X14" pad="P$3"/>
<contactref element="X7" pad="P$3"/>
<contactref element="X8" pad="P$3"/>
<contactref element="X9" pad="P$3"/>
<contactref element="X10" pad="P$3"/>
<contactref element="X17" pad="P$3"/>
<contactref element="X18" pad="P$3"/>
<contactref element="X19" pad="P$3"/>
<contactref element="X20" pad="P$3"/>
<contactref element="C10" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="X15" pad="P$3"/>
<contactref element="X16" pad="P$3"/>
<contactref element="X22" pad="2"/>
<contactref element="X2" pad="4"/>
<contactref element="X2" pad="M1"/>
<contactref element="D1" pad="GND"/>
<contactref element="SW1" pad="C"/>
<contactref element="SW1" pad="D"/>
<contactref element="X2" pad="M2"/>
<contactref element="IC5" pad="5"/>
<contactref element="U2" pad="13"/>
<contactref element="U2" pad="14"/>
<contactref element="C11" pad="1"/>
<contactref element="IC2" pad="15"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="19"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="21"/>
<contactref element="U2" pad="15"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC2" pad="5"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="5"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="47"/>
<contactref element="IC1" pad="23"/>
<contactref element="IC1" pad="44"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C22" pad="-"/>
<contactref element="C25" pad="2"/>
<contactref element="R25" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R36" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC9" pad="4"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="-12V">
<contactref element="C19" pad="-"/>
<contactref element="D4" pad="A"/>
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="25"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="C13" pad="2"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC10" pad="4"/>
<contactref element="C15" pad="2"/>
<contactref element="C27" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="D3" pad="C"/>
<contactref element="C18" pad="+"/>
<contactref element="C9" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C10" pad="1"/>
<contactref element="IC2" pad="24"/>
<contactref element="C12" pad="1"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC8" pad="2"/>
<contactref element="IC9" pad="2"/>
<contactref element="C30" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="C22" pad="+"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC10" pad="8"/>
<contactref element="C14" pad="1"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="+5V">
</signal>
<signal name="AREF_5">
<contactref element="U2" pad="18"/>
<contactref element="IC8" pad="6"/>
<contactref element="C31" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R7" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="U2" pad="6"/>
<contactref element="D1" pad="CLK"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="45"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="7"/>
<contactref element="D1" pad="MOSI"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="SS_DAC0">
<contactref element="U2" pad="5"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="CV_OUT_1">
<contactref element="X3" pad="P$1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="CV_OUT_2">
<contactref element="X4" pad="P$1"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="CV_OUT_3">
<contactref element="X5" pad="P$1"/>
<contactref element="IC2" pad="23"/>
</signal>
<signal name="CV_OUT_4">
<contactref element="X6" pad="P$1"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="GATE_OUT_1">
<contactref element="X11" pad="P$1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="D_GATE_OUT_1">
<contactref element="IC1" pad="10"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="GATE_OUT_3">
<contactref element="X13" pad="P$1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="D_GATE_OUT_3">
<contactref element="IC1" pad="12"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="GATE_OUT_2">
<contactref element="X12" pad="P$1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="D_GATE_OUT_2">
<contactref element="IC1" pad="11"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="GATE_OUT_4">
<contactref element="X14" pad="P$1"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="D_GATE_OUT_4">
<contactref element="IC1" pad="13"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="26"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="10"/>
<contactref element="IC1" pad="7"/>
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R17" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R17" pad="1"/>
<contactref element="X21" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="D2" pad="A"/>
<contactref element="X21" pad="5"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="MIDI_DATA_IN">
<contactref element="R20" pad="1"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="N$13">
<contactref element="PWR1" pad="9"/>
<contactref element="D3" pad="A"/>
<contactref element="PWR1" pad="10"/>
</signal>
<signal name="N$20">
<contactref element="D4" pad="C"/>
<contactref element="PWR1" pad="1"/>
<contactref element="PWR1" pad="2"/>
</signal>
<signal name="SS_USB">
<contactref element="IC1" pad="43"/>
</signal>
<signal name="+3V3">
<contactref element="C20" pad="+"/>
<contactref element="J1" pad="1"/>
<contactref element="R20" pad="2"/>
<contactref element="IC5" pad="8"/>
<contactref element="R18" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="D1" pad="VIN"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="48"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="17"/>
<contactref element="IC1" pad="25"/>
<contactref element="C5" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="R7" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC2" pad="14"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="INT_USB">
<contactref element="IC1" pad="21"/>
</signal>
<signal name="RST_USB">
<contactref element="IC1" pad="42"/>
</signal>
<signal name="SS_DAC1">
<contactref element="IC2" pad="7"/>
<contactref element="IC1" pad="41"/>
</signal>
<signal name="CV_OUT_5">
<contactref element="X7" pad="P$1"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="CV_OUT_6">
<contactref element="X8" pad="P$1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="CV_OUT_7">
<contactref element="X9" pad="P$1"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="CV_OUT_8">
<contactref element="X10" pad="P$1"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="CV_OUT_9">
<contactref element="X17" pad="P$1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="CV_OUT_10">
<contactref element="X18" pad="P$1"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="CV_OUT_11">
<contactref element="X19" pad="P$1"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="CV_OUT_12">
<contactref element="X20" pad="P$1"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="MIDI_DATA_OUT">
<contactref element="R16" pad="1"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="6"/>
<contactref element="X1" pad="P$1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="5"/>
<contactref element="X1" pad="P$2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R10" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="IC10" pad="1"/>
</signal>
<signal name="GATE_OUT_6">
<contactref element="X16" pad="P$1"/>
<contactref element="R37" pad="1"/>
</signal>
<signal name="D_GATE_OUT_5">
<contactref element="IC1" pad="14"/>
<contactref element="R34" pad="2"/>
</signal>
<signal name="D_GATE_OUT_6">
<contactref element="IC1" pad="15"/>
<contactref element="R38" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="X22" pad="5"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R18" pad="1"/>
<contactref element="X22" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="X2" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="X2" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="USB_PER_D_N">
<contactref element="R2" pad="2"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="USB_PER_D_P">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="SS_OLED">
<contactref element="D1" pad="CCS"/>
<contactref element="IC1" pad="20"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="ENC_A">
<contactref element="SW1" pad="A"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="ENC_B">
<contactref element="SW1" pad="B"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="ENC_SW">
<contactref element="SW1" pad="E"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="SDC_OLED">
<contactref element="D1" pad="SDC"/>
<contactref element="IC1" pad="46"/>
</signal>
<signal name="N$12">
<contactref element="IC5" pad="7"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R6" pad="1"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="AREF_25">
<contactref element="IC2" pad="17"/>
<contactref element="IC9" pad="6"/>
<contactref element="C32" pad="1"/>
</signal>
<signal name="JTMS">
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="JTCK">
<contactref element="J1" pad="4"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="JTDO">
<contactref element="J1" pad="6"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="JTDI">
<contactref element="J1" pad="8"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="RST_OLED">
<contactref element="D1" pad="RES"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="RST_DAC0">
<contactref element="U2" pad="17"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$16">
<contactref element="R24" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="IC10" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R23" pad="1"/>
<contactref element="IC10" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="R11" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="IC10" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="IC10" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="R12" pad="1"/>
<contactref element="IC10" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="R15" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="IC7" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R26" pad="1"/>
<contactref element="IC7" pad="3"/>
</signal>
<signal name="N$26">
<contactref element="R29" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="IC7" pad="7"/>
</signal>
<signal name="N$27">
<contactref element="R31" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="IC7" pad="6"/>
</signal>
<signal name="N$28">
<contactref element="R30" pad="1"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="N$29">
<contactref element="R33" pad="2"/>
<contactref element="R35" pad="1"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R35" pad="2"/>
<contactref element="R36" pad="1"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="R34" pad="1"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="R37" pad="2"/>
<contactref element="R39" pad="1"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="R39" pad="2"/>
<contactref element="R40" pad="1"/>
<contactref element="IC4" pad="6"/>
</signal>
<signal name="N$34">
<contactref element="R38" pad="1"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="N$35">
<contactref element="R33" pad="1"/>
<contactref element="X15" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="PWR1" pad="7"/>
<contactref element="PWR1" pad="5"/>
<contactref element="PWR1" pad="3"/>
<contactref element="C18" pad="-"/>
<contactref element="C19" pad="+"/>
<contactref element="PWR1" pad="4"/>
<contactref element="PWR1" pad="6"/>
<contactref element="PWR1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
