<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="ABRACON_ABM3B-16.000MHZ-B2-T_0">
                    <description>XTAL-1-3-4</description>
                </package>
            </packages>
            <symbols>
                <symbol name="ABRACON_ABM3B-16.000MHZ-B2-T_0_0">
                    <description>XTAL-1-3-4</description>
                    <pin direction="pas" name="X1"/>
                    <pin direction="pas" name="X2"/>
                    <pin direction="pwr" name="1_GND"/>
                    <pin direction="pwr" name="2_GND"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="X" name="ABRACON_ABM3B-16.000MHZ-B2-T">
                    <description>XTAL-1-3-4</description>
                    <gates>
                        <gate name="G$0" symbol="ABRACON_ABM3B-16.000MHZ-B2-T_0_0"/>
                    </gates>
                    <devices>
                        <device name="ABRACON_ABM3B-16.000MHZ-B2-T_0_0" package="ABRACON_ABM3B-16.000MHZ-B2-T_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="X1"/>
                                <connect gate="G$0" pad="2" pin="1_GND"/>
                                <connect gate="G$0" pad="3" pin="X2"/>
                                <connect gate="G$0" pad="4" pin="2_GND"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="Package_Quantity" value="500"/>
                                    <attribute name="Package_Description" value="4-Pin Surface Mount Device, Body 5 x 3.2 mm"/>
                                    <attribute name="ciiva_ids" value="780013"/>
                                    <attribute name="Component_Link_1_Description" value="Manufacturer URL"/>
                                    <attribute name="vault_guid" value="1D2E735F-7538-4E5D-94A5-F115CCB61288"/>
                                    <attribute name="Width" value="0.197 inch"/>
                                    <attribute name="Min_Operating_Temperature" value="-40degC"/>
                                    <attribute name="Tolerance" value="30%"/>
                                    <attribute name="MPN" value="ABM3B-16.000MHZ-B2-T"/>
                                    <attribute name="Packaging" value="Tape and Reel"/>
                                    <attribute name="Component_Link_1_URL" value="http://www.abracon.com/"/>
                                    <attribute name="Shielding" value="Shielded"/>
                                    <attribute name="prefix" value="X"/>
                                    <attribute name="import_ts" value="1521851067"/>
                                    <attribute name="Datasheet_Version" value="Aug-15"/>
                                    <attribute name="Ro_HSCompliant" value="true"/>
                                    <attribute name="Max_Operating_Temperature" value="105degC"/>
                                    <attribute name="datasheet" value="http://www.abracon.com/Resonators/abm3b.pdf"/>
                                    <attribute name="vault_revision" value="9E217A51-3453-441B-A0BB-14CA7588F9CB"/>
                                    <attribute name="Mount" value="Surface Mount"/>
                                    <attribute name="footprint_variant_name_0" value="Manufacturer Recommended"/>
                                    <attribute name="release_date" value="1475110299"/>
                                    <attribute name="REACH_SVHC" value="Unknown"/>
                                    <attribute name="Package_Reference" value="ABM3B"/>
                                    <attribute name="imported_from" value="vault"/>
                                    <attribute name="imported" value="yes"/>
                                    <attribute name="Current_Rating" value="1.82 A"/>
                                    <attribute name="Length" value="0.197 inch"/>
                                    <attribute name="Height" value="2.8 mm"/>
                                    <attribute name="resistance" value="0.033 Ohm"/>
                                    <attribute name="MF" value="Abracon"/>
                                    <attribute name="package" value="5028"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
