<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="ABRACON_ABM3B-12.000MHZ-B2-T_0">
                    <description>XTAL-1-3-4</description>
                </package>
            </packages>
            <symbols>
                <symbol name="ABRACON_ABM3B-12.000MHZ-B2-T_0_0">
                    <description>XTAL-1-3-4</description>
                    <pin direction="pas" name="X1"/>
                    <pin direction="pas" name="X2"/>
                    <pin direction="pwr" name="1_GND"/>
                    <pin direction="pwr" name="2_GND"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="X" name="ABRACON_ABM3B-12.000MHZ-B2-T">
                    <description>XTAL-1-3-4</description>
                    <gates>
                        <gate name="G$0" symbol="ABRACON_ABM3B-12.000MHZ-B2-T_0_0"/>
                    </gates>
                    <devices>
                        <device name="ABRACON_ABM3B-12.000MHZ-B2-T_0_0" package="ABRACON_ABM3B-12.000MHZ-B2-T_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="X1"/>
                                <connect gate="G$0" pad="2" pin="1_GND"/>
                                <connect gate="G$0" pad="3" pin="X2"/>
                                <connect gate="G$0" pad="4" pin="2_GND"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="Package_Quantity" value="500"/>
                                    <attribute name="Package_Description" value="4-Pin Surface Mount Device, Body 5 x 3.2 mm"/>
                                    <attribute name="ciiva_ids" value="780008"/>
                                    <attribute name="Component_Link_1_Description" value="Manufacturer URL"/>
                                    <attribute name="vault_guid" value="24D0D680-39A5-4850-90ED-8111495D22A7"/>
                                    <attribute name="Dropout_Voltage" value="2 V"/>
                                    <attribute name="Pins" value="3"/>
                                    <attribute name="Min_Operating_Temperature" value="0 degC"/>
                                    <attribute name="MPN" value="ABM3B-12.000MHZ-B2-T"/>
                                    <attribute name="Packaging" value="Tape and Reel"/>
                                    <attribute name="Component_Link_1_URL" value="http://www.abracon.com/"/>
                                    <attribute name="imported" value="yes"/>
                                    <attribute name="Datasheet_Version" value="Aug-15"/>
                                    <attribute name="Outputs" value="1"/>
                                    <attribute name="prefix" value="X"/>
                                    <attribute name="import_ts" value="1521842082"/>
                                    <attribute name="Case_Package" value="TO-263-4"/>
                                    <attribute name="Ro_HSCompliant" value="true"/>
                                    <attribute name="Max_Operating_Temperature" value="125 degC"/>
                                    <attribute name="Max_Input_Voltage" value="25 V"/>
                                    <attribute name="Output_Voltage" value="5 V"/>
                                    <attribute name="vault_revision" value="F364169E-CEC8-420F-9568-55648A1B8707"/>
                                    <attribute name="Mount" value="Surface Mount"/>
                                    <attribute name="footprint_variant_name_0" value="Manufacturer Recommended"/>
                                    <attribute name="release_date" value="1475124701"/>
                                    <attribute name="REACH_SVHC" value="No SVHC"/>
                                    <attribute name="Nominal_Output_Voltage" value="5 V"/>
                                    <attribute name="imported_from" value="vault"/>
                                    <attribute name="datasheet" value="http://www.abracon.com/Resonators/abm3b.pdf"/>
                                    <attribute name="Min_Input_Voltage" value="7 V"/>
                                    <attribute name="Weight" value="0.050897 oz"/>
                                    <attribute name="Max_Ouput_Current" value="1.5 A"/>
                                    <attribute name="Radiation_Hardening" value="No"/>
                                    <attribute name="MF" value="Abracon"/>
                                    <attribute name="package" value="ABM3B"/>
                                    <attribute name="Output_Current" value="1.5 A"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
